Preparing U-Boot | Qt 5.12

- Qt 5.12
- Preparing U-Boot
- Qt 5.12.10 Reference Documentation

Creating Bootable SD Card ◦ Qt for INTEGRITY: Monolith Project Tutorial

# Preparing U-Boot

Finally, prepare the i.MX6 Quad board for U-Boot:

1. Connect to your i.MX6 Quad board with a serial connection at a baud rate of 115200.
2. Set the following environment variables in the U-Boot terminal:

        setenv bootcmd_demo_dt 'mmc dev 1;
        fatload mmc 1:1 20000000 demo.image;
        fatload mmc 1:1 4FFE0000 imx6q-sabrelite.dtb;
        bootm 20000000 - 4FFE0000'

        setenv bootcmd 'run bootcmd_demo_dt'
        saveenv

   Note: The file demo.image was built with the mkimage tool in Building U-Boot Image.

3. Reset the i.MX6 Quad board.

Now your i.MX6 Quad board is ready to run your application.

Creating Bootable SD Card ◦ Qt for INTEGRITY: Monolith Project Tutorial