Qt for QNX | Qt 5.13

Qt 5.13 | Qt for QNX

Qt 5.13.2 Reference Documentation

# Qt for QNX

## Supported Architectures and QNX Releases

From the perspective of an application development platform, Qt runs on top of QNX Neutrino RTOS. System integrators and application developers use a QNX SDP (Software Development Platform) which includes QNX Neutrino RTOS components for various targets and a full set of development tools.

Qt 5 is currently tested and supported on QNX SDP 7.0, with support for both 32-bit and 64-bit target architectures:

- `ARMle-v7` and `x86` (32-bit)
- `AArch64le` and `x86-64` (64-bit)

Support for 64-bit architectures was added in QNX SDP 7.0.

### Previous Releases

Older QNX SDP releases and other architectures may also work, but are not subject to regular builds and testing.

- Qt for QNX SDP 6.6

For a specific list of available boards, displays and input devices, contact QNX Software Systems (info@qnx.com) or KDAB (qnx-info@kdab.com). Qt on the QNX Neutrino OS is also supported by Qt for Device Creation, contact The Qt Company for more details.

## Supported Modules

All the Qt Essentials modules are supported in Qt for QNX.

See Qt Add-Ons for information about which Qt Add-Ons modules are supported in Qt for QNX.

If you build Qt from a released source code distribution archive, the `configure` tool ensures that the build will be made only for modules which are known to build for the target specified. Additionally, you can explicitly exclude unsupported or not needed modules from the build via the `-skip <module>` option when running the `configure` tool.

If you build Qt directly from the Git repository, you should initialize the repository only with modules which are supported or build and install modules separately. This helps to prevent unexpected build problems.

## Build Requirements

Building Qt 5 requires the following packages available from the QNX website (registration required for access to downloads):

- QNX SDP 7.0 with http://www.qnx.com/download/group.html?programid=26808

The compiler and other parts of the tool chain are provided in the SDP packages. You do not need any additional installations on your host PC. However, it is advisable to ensure that you can build Qt for the desktop target on the host as well. See Building Qt Sources for more details. All supported QNX Neutrino RTOS targets are fully integrated in the makespecs provided in the Qt sources.

You need to specify the target name for cross-compilation when configuring a Qt build:

Architecture | Configure cross-compilation target
--- | ---

`ARMle-v7` (32-bit)

      ./configure -xplatform qnx-armle-v7-qcc

`AArch64le` (64-bit)

      ./configure -xplatform qnx-aarch64le-qcc

`x86` (32-bit)

      ./configure -xplatform qnx-x86-qcc

`x86-64` (64-bit)

      ./configure -xplatform qnx-x86-64-qcc

The `configure` tool runs various tests to detect capabilities of the SDP and its add-ons. It sets related flags according the test results. Check the configure summary on the console or in `./qtbase/config.summary` if needed and set other flags manually as required.

Independent of the platform you are building for, consider using the `-prefix` option with `configure` as well, for example, `-prefix<Qt-install-path>`. This specifies the target folder where Qt will be installed and places all build artifacts outside of the source code tree.

See Qt Configure Options for more details.

## Qt Runtime Target Requirements

QNX Software Systems delivers software solutions for making embedded devices. This includes creation of QNX Neutrino RTOS boot images in a very flexible way. Even though QNX provides several reference scripts for the OS image creation, sooner or later you will need to make changes or you might decide to create an OS image from scratch. Qt relies on the existence of several third-party components and selected OS services. Due to this, QNX Neutrino RTOS boot images for a target device running Qt must meet a couple of requirements to ensure that Qt works as expected. The sections below list the crucial parts for Qt.

### QNX Screen Graphics Subsystem

Before any Qt application can be started, the QNX Screen Graphics Subsystem (also called just "Screen") must be running. The Screen consists not only of a driver, but also includes several utilities and other services which are used by Qt. This includes processing of mouse and keyboard events as well. You can ensure that the Screen is configured and running correctly by verifying that a graphics application, like `gles2-gears`, can be started and runs without problems. Most of the recent sample OS build scripts in the SDP include sections with all components and start commands for the Screen. Use them as a reference.

### IPv6 Support

Qt's networking stack requires IPv6 support to be enabled, independent of whether the actual networking uses IPv4 or IPv6. That means, that `io-pkt-v6-hc` must be running, not `io-pkt-v4`.

### Random Device `/dev/random`

Qt requires `/dev/random` to be present and functional. Start it before starting any Qt application or during the system startup:

      random -p
      waitfor /dev/random

### System Logger

QNX provides the slog2 logging framework tailored to specifics of embedded systems. The major advantage of it is a much better performance than a text output to files. Qt uses this framework by default for any logging output going through QDebug on QNX Neutrino RTOS. The `slog2` service should be started during the system startup. The `slog2` also relies on the existence of the `/tmp` folder which has to be configured as well, for example:

      [type=link] /tmp=/dev/shmem
      display_msg "Starting slogger2..."
      slogger2 -U1001:1000 &
      waitfor /dev/slog2

### Environment Variables

There is a set of environment variables you should set when starting a Qt application. Most of them are actually not specific to QNX Neutrino RTOS. They are still mentioned here, since knowing them just saves a lot of time in case of problems.

#### Qt Runtime Location

If you did not build Qt with RPATH enabled, you can place the Qt runtime components in any folder in the file system. The following environment variables should point to valid locations assuming that the Qt installation is located in `<Qt-install-path>`:

- `LD_LIBRARY_PATH` should contain the path to the Qt libraries in `<Qt-install-path>/lib`
- `QT_PLUGIN_PATH` defines where the Qt plug-ins are located. It should be set to `<Qt-install-path>/plugins`
- `QML2_IMPORT_PATH` defines where the Qt Quick plug-ins are located. It should be set to `<Qt-install-path>/qml`
- If Qt does not use fontconfig, you must either provide the path to the fonts with `QT_QPA_FONTDIR`, or place the fonts under `<Qt-install-path>/lib/fonts` which is the default font location.

#### Physical Screen Size

Qt needs information about the physical dimensions of the attached display to determine DPI values and thus set correct font sizes. Usually, this information is provided by the Screen. In some cases you may see an invalid screen size such as 0mmx0mm. In such a case Qt requires an environment variable `QQNX_PHYSICAL_SCREEN_SIZE` set to according values to get the required information. If Qt applications exit with an error message saying that the physical screen size couldn't be determined, set the variable like this before starting the Qt application:

      export QQNX_PHYSICAL_SCREEN_SIZE=150,100

to inform Qt that the screen has a width of 150mm and a height of 100mm in this particular case. The physical screen size is measured in millimeters (mm) and should correspond to the actual physical size of the display in the final configuration.

#### Troubleshooting the First Start of a Qt Application

The only drawback of the flexibility provided by QNX Neutrino RTOS is a risk that the run environment is slightly different on your target than what is expected by Qt. This is a common reason why a Qt application on a new target fails to start. A few generic environment variables can help locate the root cause for problems:

- Setting `QT_DEBUG_PLUGINS` to `1` helps to see why the QPA plugin cannot load.
- Setting `LD_DEBUG` to `1` helps to see where and how shared libraries are loaded. This can be used in combination with `QT_DEBUG_PLUGINS` when a plugin failed to load because it could not load other shared libraries.
- Setting `QT_LOGGING_TO_CONSOLE` will force sending all logging messages to `stderr` instead of `slog2`. This is useful for analyzing application startup problems, as you do not need to use another tool to see the messages.

### Third Party Libraries

Make sure that your system image contains the following additional 3rd-party libraries which are not always included in minimal QNX Neutrino RTOS images:

- `libfontconfig`
- `libfreetype`
- `libiconv`
- `libicui18n`
- `libicudata`
- `libicuuc`
- `libpng14`
- `libxml2`
- `libsqlite3`
- `libssl`
- `libcrypto`

Note: This is not a complete list of shared libraries used by Qt on QNX Neutrino OS. Multiple shared libraries are already available in a typical OS image, or included by other parts of the system, for example, the `Screen`.

### Accessing Environment Variables

`setconf` and `getconf` are required to access POSIX environment variables, especially for the host name and time and date.

## Qt Creator Target Requirements

A QNX Neutrino RTOS target used for development with Qt Creator should provide a few additional command line tools and services.

### SSH

Deployment and remote application startup relies on SSH. The SSH daemon (`sshd`) must be installed and running during the system startup. Please note that it requires `/dev/random` which was already mentioned. It also expects specific access rights to be set correctly to its configuration files. The latter makes it impossible starting SSH from a file system which does not have full access rights support, for example, FAT.

### SCP and SFTP

`scp` and `sftp` utilities are used by Qt Creator for deployment and should be available on the target. Additionally, `inetd` daemon has to be started at the system startup which then launches according services, including FTP when needed.

### QNX Tools for Remote Debugging

Remote debugging requires the `pdebug` (process-level debugger) to be running on the development device. It is usually started by the `qconn` process which also provides various process information to Qt Creator. Generally, Qt Creator uses the same remote debugging interfaces as the QNX Momentics IDE provided in the SDP. See the related QNX documentation for more details.

### Other Utilities on the Target Device

QNX provides board support packages (BSPs) for many common platforms and their individual variants. However, if you need a BSP for a board that QNX does not provide, you can modify an existing one or develop your own.

When you develop a BSP for your board, you should include the following utilities to enable Qt Creator to deploy, run, debug, and stop applications on QNX devices:

- `awk`
- `cat`
- `cut`
- `df`
- `grep`
- `kill`
- `ln`
- `mkdir`
- `netstat`
- `print`
- `printf`
- `ps`
- `read`
- `sed`
- `sleep`
- `slog2info`
- `tail`
- `tar`
- `zip`
- `uname`
- `unzip`

The utilities need to be in a standard location, such as `/bin` or `/usr/bin`. Alternatively, you can use the `~/.ssh/environment` file to set variables for remote commands, such as `PATH`. In addition, you must set `enable PermitUserEnvironment` in the SSH Daemon configuration.

Run the test when you configure a new target device in Qt Creator to verify that all required components are available and running.

For more information about modifying or developing a BSP for you board, see Customizing a BSP in the QNX developer documentation.

### Deployment Destination Folder

Qt Creator deploys an application to the target device before starting it remotely. On most embedded devices, it is just copying application binaries and related data files to a folder on the target device. However, there is no standard for how this folder is called and where it is located. Quite a few configurations use `/tmp` for this, which is often mapped to a RAM disk. This can cause some confusion as deployed applications disappear on the next device shutdown.

Another popular target is `/opt`. This folder is located in a read-only partition on many systems, making deployment impossible. Make sure that you use a destination folder which meets your needs. You can set it in the `install.path` variable in the `.pro` file of your project, see Installing Files in the qmake documentation for more details.