xyseriesiodevice.cpp Example File | Qt Charts 5.11

Qt 5.11 | Qt Charts | Audio Example | xyseriesiodevice.cpp Example File

Qt Charts | Commercial or GPLv3

# xyseriesiodevice.cpp Example File

audio/xyseriesiodevice.cpp

      /****************************************************************************
      **
      ** Copyright (C) 2016 The Qt Company Ltd.
      ** Contact: https://www.qt.io/licensing/
      **
      ** This file is part of the Qt Charts module of the Qt Toolkit.
      **
      ** $QT_BEGIN_LICENSE:GPL$
      ** Commercial License Usage
      ** Licensees holding valid commercial Qt licenses may use this file in
      ** accordance with the commercial license agreement provided with the
      ** Software or, alternatively, in accordance with the terms contained in
      ** a written agreement between you and The Qt Company. For licensing terms
      ** and conditions see https://www.qt.io/terms-conditions. For further
      ** information use the contact form at https://www.qt.io/contact-us.
      **
      ** GNU General Public License Usage
      ** Alternatively, this file may be used under the terms of the GNU
      ** General Public License version 3 or (at your option) any later version
      ** approved by the KDE Free Qt Foundation. The licenses are as published by
      ** the Free Software Foundation and appearing in the file LICENSE.GPL3
      ** included in the packaging of this file. Please review the following
      ** information to ensure the GNU General Public License requirements will
      ** be met: https://www.gnu.org/licenses/gpl-3.0.html.
      **
      ** $QT_END_LICENSE$
      **
      ****************************************************************************/

      #include "xyseriesiodevice.h"

      #include <QtCharts/QXYSeries>

      XYSeriesIODevice::XYSeriesIODevice(QXYSeries *series, QObject *parent) :
          QIODevice(parent),
          m_series(series)
      {
      }

      qint64 XYSeriesIODevice::readData(char *data, qint64 maxSize)
      {
          Q_UNUSED(data)
          Q_UNUSED(maxSize)
          return -1;
      }

      qint64 XYSeriesIODevice::writeData(const char *data, qint64 maxSize)
      {
          static const int resolution = 4;

          if (m_buffer.isEmpty()) {
              m_buffer.reserve(sampleCount);
              for (int i = 0; i < sampleCount; ++i)
                  m_buffer.append(QPointF(i, 0));
          }

          int start = 0;
          const int availableSamples = int(maxSize) / resolution;
          if (availableSamples < sampleCount) {
              start = sampleCount - availableSamples;
              for (int s = 0; s < start; ++s)
                  m_buffer[s].setY(m_buffer.at(s + availableSamples).y());
          }

          for (int s = start; s < sampleCount; ++s, data += resolution)
              m_buffer[s].setY(qreal(uchar(*data) -128) / qreal(128));

          m_series->replace(m_buffer);
          return (sampleCount - start) * resolution;
      }