Qt for Embedded Linux | Qt 5.13

Qt 5.13 | Qt for Embedded Linux

Qt 5.13.1 Reference Documentation

# Qt for Embedded Linux

On Embedded Linux systems, there are multiple platform plugins that you can use: EGLFS, LinuxFB, DirectFB, or Wayland. However, the availability of these plugins depend on how Qt is configured.

EGLFS is the default plugin on many boards. If it's not suitable, use the `QT_QPA_PLATFORM` environment variable to request another plugin. Alternatively, for quick tests, use the `-platform` command-line argument with the same syntax.

Note: As of Qt 5.0, Qt no longer has its own window system (QWS) implementation. For single-process use cases, the Qt Platform Abstraction is a superior solution; multi-process use cases are supported through Wayland.

## Platform Plugins for Embedded Linux Devices

### EGLFS

EGL is an interface between OpenGL and the native windowing system. Qt can use EGL for context and surface management, however the API contains no platform-specifics. Creating a native window, which won't necessarily be an actual window on the screen, must still be done by platform-specific means. This is why we need the board or GPU-specific adaptation code. Typically, these adaptations are provided as:

- EGLFS hooks -- a single source file compiled into the platform plugin
- EGL device integration -- dynamically loaded plugins

EGLFS is a platform plugin for running Qt5 applications on top of EGL and OpenGL ES 2.0, without an actual windowing system like X11 or Wayland. In addition to Qt Quick 2 and native OpenGL applications, EGLFS supports software-rendered windows, like QWidget, too. For QWidget, the widgets' contents are rendered using the CPU into images, which are then uploaded into textures and composited by the plugin.

EGLFS is the recommended plugin for modern Embedded Linux devices that include a GPU.

EGLFS forces the first top-level window - either a QWidget or a QQuickView - to become fullscreen. This window is also chosen to be the root widget window into which all other top-level widgets are composited. For example, dialogs, popup menus, or combo boxes. This behavior is necessary because with EGLFS there is always exactly one native window and one EGL window surface; these belong to the widget or window that is created first. This approach works well when there is a main window that exists for the application's lifetime and all other widgets are either non top-levels or are created afterwards, once the main window is shown.

There are further restrictions for OpenGL-based windows. EGLFS supports a single single fullscreen GL window (as of Qt 5.3), like OpenGL-based QWindow, a QQuickView, or a QOpenGLWidget. Opening additional OpenGL windows or mixing such windows with QWidget-based content isn't supported; Qt terminates the application with an error message.

If necessary, `eglfs` can be configured using the following environment variables:

Environment Variable | Description
--- | ---

`QT_QPA_EGLFS_INTEGRATION`

In addition to the compiled-in hooks, it is also possible to use dynamically loaded plugins to provide device or vendor-specific adaptation. This environment variable enforces a specific plugin. For example, setting it to eglfs_kms uses the KMS/DRM backend. This is only an option when no static or compiled-in hooks were specified in the device makespecs. In practice, the traditional compiled-in hooks are rarely used, almost all backends are now migrated to plugins. The device makespecs still contain a relevant `EGLFS_DEVICE_INTEGRATION` entry: the name of the preferred backend for that particular device. This is optional, but very useful to avoid the need to set this environment variable if there are more than one plugin present in the target system. In a desktop environment the KMS or X11 backends are prioritized, depending on the presence of the `DISPLAY` environment variable.

Note: On some boards a special value of `none` is used instead of an actual plugin. This indicates that no special integration is necessary to use EGL with the framebuffer; no plugins must be loaded.

`QT_QPA_EGLFS_PHYSICAL_WIDTH` and `QT_QPA_EGLFS_PHYSICAL_HEIGHT` | Specifies the physical screen's width and height in millimeters. On platforms where the value can't be queried from the framebuffer device /dev/fb0 or via other means, a default DPI of 100 is used. Use this variable to override any such defaults. Setting this variable is important because QWidget- or Qt Quick Controls-based applications rely on these values. Running these applications with the hard-coded settings may result in user interface elements with sizes that are unsuitable for the display in use.
`QT_QPA_EGLFS_ROTATION` | Specifies the rotation applied to software-rendered content in QWidget-based applications. Supported values are 180, 90, and -90. This variable does not apply to OpenGL-based windows, including Qt Quick. Qt Quick applications can apply transformations in their QML scene instead. The standard `eglfs` mouse cursor always takes the value into account, with an appropriately positioned and rotated pointer image, regardless of the application type. However, special cursor implementations, such as the KMS/DRM backend's hardware cursor, may not support rotation.
`QT_QPA_EGLFS_FORCEVSYNC` | When set, `eglfs` requests `FBIO_WAITFORVSYNC` on the framebuffer device after each call to eglSwapBuffers(). This variable is only relevant for backends relying on the legacy Linux `fbdev` subsystem. Normally, with a default swap interval of 1, Qt assumes that calling eglSwapBuffers() takes care of vsync; if it doesn't (for example, due to driver bugs), try setting `QT_QPA_EGLFS_FORCEVSYNC` to a non-zero value.
`QT_QPA_EGLFS_FORCE888` | When set, the red, green, and blue color channel sizes are ignored when `eglfs` creates a new context, window or offscreen surface. Instead, the plugin requests a configuration with 8 bits per channel. This can be helpful on devices where configurations with less than 32 or 24 bits per pixel (for example, 5-6-5 or 4-4-4) are chosen by default despite knowing they are not ideal, for example, due to banding effects. Instead of changing application code, this variable provides a shortcut to force 24 or 32 bpp configurations.

Additionally, the following less commonly used variables are available:

Environment Variable | Description
--- | ---
`QT_QPA_EGLFS_FB` | Overrides the framebuffer device. The default is `/dev/fb0`. On most embedded platforms this variable isn't very relevant because the framebuffer is used only to query settings like the display dimensions. However, on certain devices, this variable provides the ability to specify which display to use in multiple display setups, similar to the `fb` parameter in LinuxFB.
`QT_QPA_EGLFS_WIDTH` and `QT_QPA_EGLFS_HEIGHT` | Contains the screen's width and height in pixels. While `eglfs` tries to determine the dimensions from the framebuffer device /dev/fb0, this doesn't always work. It may be necessary to manually specify the sizes.
`QT_QPA_EGLFS_DEPTH` | Overrides the color depth for the screen. On platforms where the framebuffer device /dev/fb0 is not available or the query is not successful, a default of `32` is used. Use this variable to override any such defaults. Note: This variable only affects the color depth value reported by QScreen. It has no connection to EGL configurations and the color depth used for OpenGL rendering.
`QT_QPA_EGLFS_SWAPINTERVAL` | By default, a swap interval of `1` is requested. This variable enables synchronizing to the display's vertical refresh. Use this variable to override the swap interval's value. For instance, passing 0 disables blocking on swap, resulting in running as fast as possible without any synchronization.
`QT_QPA_EGLFS_DEBUG` | When set, some debugging information is printed on the debug output. For example, the input QSurfaceFormat and the properties of the chosen EGL configuration are printed while creating a new context. When used together with Qt Quick's `QSG_INFO` variable, you can get useful information for troubleshooting issues related to the EGL configuration.

In addition to `QT_QPA_EGLFS_DEBUG`, `eglfs` also supports Qt's modern categorized logging system. The following logging categories are available:

- `qt.qpa.egldeviceintegration` – Enables logging for dynamically loaded backends. Use this category to check what backend is in use.
- `qt.qpa.input` – Enables debug output both from the `evdev` and `libinput` input handlers. Use this category to check if a given input device was recognized and opened.
- `qt.qpa.eglfs.kms` – Enables verbose logging in the KMS/DRM backend.

After running `configure`, make sure to inspect its output. This is the easiest, quickest way to identify whether you have the necessary EGLFS backend, libudev, or libinput enabled. In short, if there's an undesired "no" in your `configure` output, run:

      ./configure -v

to turn on the verbose output, so that you can see the compiler and linker invocations for each configure test.

Note: If you encounter errors about missing headers, libraries, or seemingly cryptic linker failures, often, they are a sign of an incomplete or broken sysroot and isn't related to Qt.

As an example, when targeting the Raspberry Pi with the Broadcom proprietary graphics drivers, the output should contain something like the following:

      QPA backends:
      EGLFS ................................ yes
      EGLFS details:
        EGLFS i.Mx6 ........................ no
        EGLFS i.Mx6 Wayland ................ no
        EGLFS EGLDevice .................... no
        EGLFS GBM .......................... no
        EGLFS Mali ......................... no
        EGLFS Rasberry Pi .................. yes
        EGL on X11 ......................... no

If this is not the case, it's not advisable to proceed further with the build since accelerated graphics won't be functional without the Raspberry Pi-specific backend, even if the rest of Qt compiles successfully.

### LinuxFB

This plugin writes directly to the framebuffer via Linux's fbdev subsystem. Only software-rendered content is supported. Note that on some setups the display performance is expected to be limited.

However, since fbdev is being deprecated in the Linux kernel, the DRM dumb buffer support is also available, as of Qt 5.9. To use it, set the `QT_QPA_FB_DRM` environment variable to a non-zero value. When set, provided that dumb buffers are supported by your system, legacy framebuffer devices like `/dev/fb0` won't be accessed. Instead, the rendering is set up via the DRM APIs, similar to the `eglfs_kms` backend in EGLFS. The output is double-buffered and page flipped, providing proper vsync for software-rendered content as well.

Note: When dumb buffers are in use, none of the options described below are applicable since properties like physical and logical screen sizes are all queried automatically.

The `linuxfb` plugin allows you to specify additional settings via the `QT_QPA_PLATFORM` environment variable or `-platform` command-line option. For example, `QT_QPA_PLATFORM=linuxfb:fb=/dev/fb1` specifies that the framebuffer device `/dev/fb1` must be used instead of the default `fb0`. To specify multiple settings, separate the mwith a colon (:).

Settings | Description
--- | ---
`fb=/dev/fbN` | Specifies the framebuffer devices. On multiple display setups, this setting allows you to run the application on different displays. Currently, there's no way to use multiple framebuffers from one Qt application.
`size=`<width>`x`<height> | Specifies the screen size in pixels. The plugin tries to query the display dimensions, both physical and logical, from the framebuffer device. However, this query may not always lead to proper results; it may be necessary to specify the values explicitly.
`mmsize=`<width>`x`<height> | Specifies the physical width and height in millimeters.
`offset=`<width>`x`<height> | Specifies the top-left corner of the screen offset in pixels. The default position is at `(0, 0)`.
`nographicsmodeswitch` | Specifies not to switch the virtual terminal to graphics mode (`KD_GRAPHICS`). Typically, enabling graphics mode disables the blinking cursor and screen blanking. However, when this parameter is set, those two features are also skipped.
`tty=/dev/ttyN` | Overrides the virtual console. Only used when `nographicsmodeswitch` isn't set.

As of Qt 5.9, the behavior of EGLFS and LinuxFB have been synchronized, with regards to the window sizing policy: the first top-level window is forced to cover the entire screen, with both platform plugins. If this is not desired, set the `QT_QPA_FB_FORCE_FULLSCREEN` environment variable to `0` to restore the behavior from earlier Qt versions.

## Input

When no windowing system is present, the mouse, keyboard, and touch input are read directly via `evdev` or using helper libraries such as `libinput` or `tslib`. Note that this requires that device nodes `/dev/input/event*` are readable by the user. `eglfs` and `linuxfb` have all the input handling code compiled-in.

### Using libinput

libinput is a library to handle input devices. It offers an alternative to the Qt's own `evdev` input support. To enable using `libinput`, make sure the development files for `libudev` and `libinput` are available when configuring and building Qt. `xkbcommon` is also necessary if keyboard support is desired. With `eglfs` and `linuxfb` no further actions are necessary as these plugins use `libinput` by default. If `libinput` support is not available or the environment variable `QT_QPA_EGLFS_NO_LIBINPUT` is set, Qt's own evdev handlers come in to play.

### Input on eglfs and linuxfb without libinput

Parameters like the device node name can be set in the environment variables `QT_QPA_EVDEV_MOUSE_PARAMETERS`, `QT_QPA_EVDEV_KEYBOARD_PARAMETERS` and `QT_QPA_EVDEV_TOUCHSCREEN_PARAMETERS`. Separate the entries with colons. These parameters act as an alternative to passing the settings in the `-plugin` command-line argument, and with some backends they are essential: eglfs and linuxfb use built-in input handlers so there is no separate `-plugin` argument in use.

Additionally, the built-in input handlers can be disabled by setting `QT_QPA_EGLFS_DISABLE_INPUT` or `QT_QPA_FB_DISABLE_INPUT` to `1`.

### Mouse

The mouse cursor shows up whenever `QT_QPA_EGLFS_HIDECURSOR` (for eglfs) or `QT_QPA_FB_HIDECURSOR` (for linuxfb) is not set and Qt's libudev-based device discovery reports that at least one mouse is available. When `libudev` support is not present, the mouse cursor always show up unless explicitly disabled via the environment variable.

Hot plugging is supported, but only if Qt was configured with `libudev` support (that is, if the libudev development headers are present in the sysroot at configure time). This allows connecting or disconnecting an input device while the application is running.

The evdev mouse handler supports the following extra parameters:

- `/dev/input/...` - Specifies the name of the input device. When not given, Qt looks for a suitable device either via libudev or by walking through the available nodes.
- `nocompress` - By default, input events that do not lead to changing the position compared to the last Qt mouse event are compressed; a new Qt mouse event is sent only after a change in the position or button state. This can be disabled by setting the `nocompress` parameter.
- `dejitter` - Specifies a jitter limit. By default dejittering is disabled.
- `grab` - When 1, Qt will grab the device for exclusive use.
- `abs` - Some touchscreens report absolute coordinates and cannot be differentiated from touchpads. In this special situation pass `abs` to indicate that the device is using absolute events.

### Keyboard

The evdev keyboard handler supports the following extra parameters:

- `/dev/input/...` - Specifies the name of the input device. When not given, Qt looks for a suitable device either via libudev or by walking through the available nodes.
- `grab` - Enables grabbing the input device.
- `keymap` - Specifies the name of a custom keyboard map file.
- `enable-compose` - Enables compositing.
- `repeat-delay` - Sets a custom key repeat delay.
- `repeat-rate` - Sets a custom key repeat rate.

On Embedded Linux systems that do not have their terminal sessions disabled, the behavior on a key press can be confusing as input event is processed by the Qt application and the tty. To overcome this, the following options are available:

- EGLFS and LinuxFB attempt to disable the terminal keyboard on application startup by setting the tty's keyboard mode to `K_OFF`. This prevents keystrokes from going to the terminal. If the standard behavior needs to be restored for some reason, set the environment variable `QT_QPA_ENABLE_TERMINAL_KEYBOARD` to `1`. Note that this works only when the application is launched from a remote console (for example, via `ssh`) and the terminal keyboard input remains enabled.
- An alternative approach is to use the evdev keyboard handler's `grab` parameter by passing grab=1 in `QT_QPA_EVDEV_KEYBOARD_PARAMETERS`. This results in trying to get a grab on the input device. If the `grab` is successful, no other components in the system receive events from it as long as the Qt application is running. This approach is more suitable for applications started remotely as it does not need access to the tty device.
- Finally, for many specialized Embedded Linux images it does not make sense to have the standard terminal sessions enabled in the first place. Refer to your build environment's documentation on how to disable them. For example, when generating images using the Yocto Project, unsetting `SYSVINIT_ENABLED_GETTYS` results in having no `getty` process running, and thus no input, on any of the virtual terminals.

If the default built-in keymap is not sufficient, a different one can be specified either via the `keymap` parameter or by using the eglfs-specific loadKeymap() function. The latter allows switching the keymap at runtime. Note however that this requires using eglfs' built-in keyboard handler; it is not supported when the keyboard handler is loaded via the `-plugin` command-line parameter.

Note: Special system key combinations, such as console switching (Ctrl+Alt+Fx) or zap (Ctrl+Alt+Backspace) are not currently supported and are ignored.

To generate a custom keymap, the kmap2qmap utility can be used. This can be found in the qttools module. The source files have to be in standard Linux `kmap` format, which is understood by the kernel's `loadkeys` command. This means one can use the following sources to generate `qmap` files:

- The Linux Console Tools (LCT) project.
- Xorg X11 keymaps can be converted to the `kmap` format with the `ckbcomp` utility.
- As `kmap` files are plain-text files, they can also be hand crafted.

`kmap2qmap` is a command line program, that needs at least 2 files as parameters. The last one is the generated `.qmap` file, while all the others are parsed as input `.kmap` files. For example:

      kmap2qmap i386/qwertz/de-latin1-nodeadkeys.kmap include/compose.latin1.inc de-latin1-nodeadkeys.qmap

Note: `kmap2qmap` does not support all the (pseudo) symbols that the Linux kernel supports. When converting a standard keymap, a number of warnings will be shown regarding `Show_Registers`, `Hex_A`, and so on; these messages can safely be ignored.

### Touch

For some resistive, single-touch touch screens it may be necessary to fall back to using `tslib` instead of relying on the Linux multi-touch protocol and the event devices. For modern touch screens this is not necessary. `tslib` support can be enabled by setting the environment variable `QT_QPA_EGLFS_TSLIB` or `QT_QPA_FB_TSLIB` to 1. To change the device, set the environment variable `TSLIB_TSDEVICE` or pass the device name on the command-line. Note that the `tslib` input handler generates mouse events and supports single touch only, as opposed to `evdevtouch` which generates true multi-touch QTouchEvent events too.

The evdev touch handler supports the following extra parameters:

- `/dev/input/...` - Specifies the name of the input device. When not given, Qt looks for a suitable device either via libudev or by walking through the available nodes.
- `rotate` - On some touch screens the coordinates must be rotated, which is done by setting `rotate` to 90, 180, or 270.
- `invertx` and `inverty` - To invert the X or Y coordinates in the input events, pass `invertx` or `inverty`.

For example, doing `export QT_QPA_EVDEV_TOUCHSCREEN_PARAMETERS=/dev/input/event5:rotate=180` before launching applications results in an explicitly specified touch device and flipping the coordinates - useful when the orientation of the actual screen and the touch screen do not match.

### Pen-based tablets

The `evdevtablet` plugin provides basic support for Wacom and similar, pen-based tablets. It generates QTabletEvent events only. To enable it, pass `QT_QPA_GENERIC_PLUGINS=evdevtablet` in the environment or, alternatively, pass `-plugin evdevtablet` argument on the command-line. The plugin can take a device node parameter, for example `QT_QPA_GENERIC_PLUGINS=evdevtablet:/dev/event1`, in case the Qt's automatic device discovery (based either on libudev or a walkthrough of `/dev/input/event*`) is not functional or misbehaving.

### Debugging Input Devices

It is possible to print some information to the debug output by enabling the `qt.qpa.input` logging rule, for example by setting the `QT_LOGGING_RULES` environment variable to `qt.qpa.input=true`. This is useful for detecting which device is being used, or to troubleshoot device discovery issues.

### Using Custom Mouse Cursor Images

`eglfs` comes with its own set of 32x32 sized mouse cursor images. If these are not sufficient, a custom cursor atlas can be provided by setting the `QT_QPA_EGLFS_CURSOR` environment variable to the name of a JSON file. The file can also be embedded into the application via Qt's resource system.

For example, an embedded cursor atlas with 8 cursor images per row can be specified like the following:

      {
        "image": ":/cursor-atlas.png",
        "cursorsPerRow": 8,
        "hotSpots": [
            [7, 2],
            [12, 3],
            [12, 12],
            ...
        ]
      }

Note that the images are expected to be tightly packed in the atlas: the width and height of the cursors are decided based on the total image size and the `cursorsPerRow` setting. Atlases have to provide an image for all the supported cursors.

## Display Output

When having multiple displays connected, the level of support for targeting one or more of these from one single Qt application varies between the platform plugins and often depends on the device and its graphics stack.

### eglfs with eglfs_kms backend

When the KMS/DRM backend is in use, eglfs reports all available screens in QGuiApplication::screens(). Applications can target different screens with different windows via QWindow::setScreen().

Note: The restriction of one single fullscreen window per screen still applies. Changing screens after making the QWindow visible is not supported either. Therefore, it is essential that embedded applications make all the necessary QWindow::setScreen() calls before calling QWindow::show().

When getting started with developing on a given embedded device, it is often necessary to verify the behavior of the device and drivers, and that the connected displays are working as they should. One easy way is to use the hellowindow example. Launching it with `-platform eglfs --multiscreen --timeout` arguments shows a rotating Qt logo on each connected screen for a few seconds.

Note: Most of the configuration options described below apply to all KMS/DRM-based backends, regardless of the buffer management technology (GBM or EGLStreams).

The KMS/DRM backend also supports custom configurations via a JSON file. Set the environment variable `QT_QPA_EGLFS_KMS_CONFIG` to the name of the file to enable this. The file can also be embedded into the application via the Qt resource system. An example configuration is below:

      {
        "device": "/dev/dri/card1",
        "hwcursor": false,
        "pbuffers": true,
        "outputs": [
          {
            "name": "VGA1",
            "mode": "off"
          },
          {
            "name": "HDMI1",
            "mode": "1024x768"
          }
        ]
      }

Here we configure the specified device so that

- it will not use the hardware cursor (falls back to rendering the mouse cursor via OpenGL; by default hardware cursors are enabled as they are more efficient),
- it will back QOffscreenSurface with standard EGL pbuffer surfaces (by default this is disabled and a gbm surface is used instead),
- output on the VGA connector is disabled, while HDMI is active with a resolution of 1024x768.

Additionally, such a configuration also disables looking for a device via `libudev` and instead the specified device is used.

When `mode` is not defined, the mode that is reported as preferred by the system is chosen. The accepted values for `mode` are: `off`, `current`, `preferred`, `skip`, width`x`height, width`x`height`@`vrefresh, or a modeline string.

Specifying `current` will choose a mode with a resolution matching the current one. Due to the fact that modesetting is done only when the desired mode is actually different from the active one (unless forced via the `QT_QPA_EGLFS_ALWAYS_SET_MODE` environment variable), this value is useful to keep the current mode and any content in the planes not touched by Qt. `skip` causes the connector for the output to be ignored, just as if it was disconnected. `off` is similar, but it changes the mode as well to turn off the display.

All screens reported by the DRM layer will be treated as one big virtual desktop by default. The mouse cursor implementation will take this into account and move across the screens as expected. Although not recommended, the virtual desktop mode can be disabled by setting `separateScreens` to `false` in the configuration, if desired.

By default, the virtual desktop is formed left to right, based on the order of connectors as reported by the system. This can be changed by setting `virtualIndex` to a value starting from 0. For example, the following configuration uses the preferred resolution but ensures that the left side in the virtual desktop is the screen connected to the HDMI port, while the right side is the screen connected to the DisplayPort:

      {
        "device": "drm-nvdc",
        "outputs": [
          {
            "name": "HDMI1",
            "virtualIndex": 0
          },
          {
            "name": "DP1",
            "virtualIndex": 1
          }
        ]
      }

The order of elements in the array is not relevant. Outputs with unspecified virtual indices will be placed after the others, with the original order in the DRM connector list preserved.

To create a vertical desktop space (that is, to stack top to bottom instead of left to right), add a `virtualDesktopLayout` property after `device` with the value of `vertical`.

Note: It is recommended that all screens in the virtual desktop use the same resolution, otherwise elements like the mouse cursor may behave in unexpected ways when entering areas that only exist on one given screen.

When `virtualIndex` is not sufficient, the property `virtualPos` can be used to explicitly specify the top-left position of the screen in question. Taking the previous example and assuming a resolution of 1080p for HDMI1, the following places a second HDMI-based screen below the first one:

      {
         ...
        "outputs": [
          ...
          {
            "name": "HDMI2",
            "virtualPos": "0, 1080"
          }
        ]
      }

Note: Avoid such configurations when mouse support is desired. The mouse cursor's behavior may be unexpected with non-linear layouts. Touch should present no issues however.

In some cases the automatic querying of the physical screen size via DRM may fail. Normally the `QT_QPA_EGLFS_PHYSICAL_WIDTH` and `QT_QPA_EGLFS_PHYSICAL_HEIGHT` environment variable would be used to provide the missing values, however this is not suitable anymore when multiple screens are present. Instead, use the `physicalWidth` and `physicalHeight` properties in the `outputs` list to specify the sizes in millimeters.

Note: Different physical sizes and thus differing logical DPIs are discouraged because it may lead to unexpected issues due to some graphics stack components not knowing about multiple screens and relying solely on the first screen's values.

Each active output from the `outputs` array corresponds to one QScreen instance reported from QGuiApplication::screens(). The primary screen reported by QGuiApplication::primaryScreen() is by default the screen that gets registered first. When not using `virtualIndex`, this means the decision is based on the DRM connector order. To override this, set the property `primary` to `true` on the desired entry in the `outputs` list. For example, to ensure the screen corresponding to the VGA output will be the primary even when the system happens to report the HDMI one first, one can do the following:

      {
        "device": "/dev/dri/card0",
        "outputs": [
            { "name": "HDMI1" },
            { "name": "VGA1", "mode": "1280x720", "primary": true },
            { "name": "LVDS1", "mode": "off" }
        ]
      }

For troubleshooting it might be useful to enable debug logs from the KMS/DRM backend. To do this, enable the categorized logging rule, `qt.qpa.eglfs.kms`.

Note: In an embedded environment virtual desktops are more limited than with a full windowing system. Windows overlapping multiple screens, non-fullscreen windows and moving windows between screens should be avoided and may not function as expected.

The most common and best supported use case for a multi-screen setup is to open a dedicated QQuickWindow or QQuickView for each screen. With the default `threaded` render loop of the Qt Quick scenegraph, each of these windows will get its own dedicated render thread. This is good because the threads can be throttled independently based on vsync, and will not interfere with each other. With the `basic` loop this can get problematic and animations may degrade as a result.

As an example, discovering all connected screens and creating a QQuickView for each of them can be done like this:

      int main(int argc, char **argv)
      {
          QGuiApplication app(argc, argv);

          QVector<QQuickView *> views;
          for (QScreen *screen : app.screens()) {
              QQuickView *view = new QQuickView;
              view->setScreen(screen);
              view->setResizeMode(QQuickView::SizeRootObjectToView);
              view->setSource(QUrl("qrc:/main.qml"));
              QObject::connect(view->engine(), &QQmlEngine::quit, qGuiApp, &QCoreApplication::quit);
              views.append(view);
              view->showFullScreen();
          }

          int result = app.exec();

          qDeleteAll(views);
          return result;
      }

### Advanced eglfs_kms features

Screen cloning (mirroring) is supported as of Qt 5.11. It can be enabled by the `clones` property:

      {
        "device": "/dev/dri/card0",
        "outputs": [
            { "name": "HDMI1", "mode": "1920x1080" },
            { "name": "DP1", "mode": "1920x1080", "clones": "HDMI1" }
       ]
      }

Here the content on the display connected via DisplayPort will be the same as on the HDMI one. This is ensured by simply scanning out the same buffer on both.

Note: This can only work if the resolutions are the same, there are no incompatibilities when it comes to accepted buffer formats, and the application does not have any output on the QScreen associated with a clone destination. In practice the latter means that no QWindow associated with the QScreen in question - DP1 in the example - must ever perform a QOpenGLContext::swapBuffers() operation. It is up to the configuration and the application to ensure these.

Headless mode via DRM render nodes is supported as of Qt 5.11. This allows performing GPU compute (OpenGL compute shaders, OpenCL) or offscreen OpenGL rendering without needing DRM master privileges. In this mode applications can function even when there is already another process outputting to the screen.

Just switching `device` from `/dev/dri/card0` to `/dev/dri/renderD128` is futile on its own since there are a number of operations that cannot be performed in headless mode. Therefore, this must be combined with a `headless` property, for example:

      {
          "device": "/dev/dri/renderD128",
          "headless": "1024x768"
      }

Keep in mind that windows are still sized to match the - now virtual - screen size, hence the need for specifying a size in the `headless` property. There is also a lack of vsync-based throttling.

Once enabled, applications have two typical choices to perform offscreen rendering in headless mode:

Use an ordinary window, such as a QOpenGLWindow subclass, targeting the window's default framebuffer, meaning a `gbm_surface` in practice:

      MyOpenGLWindow w;
      w.show(); // will not actually show up on screen
      w.grabFramebuffer().save("output.png");

Or the typical offscreen approach with an extra FBO:

      QOffscreenSurface s;
      s.setFormat(ctx.format());
      s.create();
      ctx.makeCurrent(&s);
      QOpenGLFramebufferObject fbo(1024, 768);
      fbo.bind();
      ctx.functions()->glClearColor(1, 0, 0, 1);
      ctx.functions()->glClear(GL_COLOR_BUFFER_BIT);
      fbo.toImage().save("output.png");
      ctx.doneCurrent();

KMS/DRM can be used with two different DRM APIs which are legacy and atomic. The main benefit of DRM atomic API is to allow several DRM plane updates within the same renderloop, whereas legacy API would require one plane update per vsync.

Atomic API is useful when you application needs to blend content into overlays keeping all the updates within the same vsync. Still not all devices support this API and it could be unavailable on some older devices. KMS backend will by default use the legacy API, but you can enable the DRM atomic API with `QT_QPA_EGLFS_KMS_ATOMIC` environment variable set to 1.

Using a smaller framebuffer than screen resolution can also be useful. This is possible with DRM atomic using the `size` parameter in the JSON file. The example below uses a 1280x720 framebuffer on a 3840x2160 videomode :

      {
        "device": "/dev/dri/card0",
        "outputs": [
          { "name": "HDMI1", "mode": "3840x2160", "size": "1280x720", "format": "argb8888" }
        ]
      }

### eglfs with eglfs_kms_egldevice backend

This backend, typically used on Tegra devices, is similar to the KMS/DRM backend mentioned above, except that it relies on the EGLDevice and EGLStream extensions instead of GBM.

For technical details about this approach, check out this presentation.

As of Qt 5.7 this backend shares many of its internal implementation with the GBM-based backend. This means that multiple screens and the advanced configuration via `QT_QPA_EGLFS_KMS_CONFIG` are supported. Some settings, such as `hwcursor` and `pbuffers` are not applicable however.

By default the backend will automatically choose the correct EGL layer for the default plane of each output. When necessary, this can be overridden by setting the `QT_QPA_EGLFS_LAYER_INDEX` environment variable to the index of the desired layer. This approach does not currently support multiple outputs, so its usage should be limited to systems with a single screen. To see which layers are available, and to debug potential startup issues, enable the logging category `qt.qpa.eglfs.kms`.

In some cases it may be necessary to perform a video mode set on application startup even when the screen reports that the desired resolution is already set. This is normally optimized away, but if the screen stays powered down, try setting the environment variable `QT_QPA_EGLFS_ALWAYS_SET_MODE` to a non-zero value and relaunch the application.

To configure the behavior of the EGLStream object used by the backend, use the `QT_QPA_EGLFS_STREAM_FIFO_LENGTH` environment variable. This assumes that `KHR_stream_fifo` is supported by the target system. By default the stream operates in mailbox mode. To switch to FIFO mode, set a value of 1 or greater. The value specifies the maximum number of frames the stream can hold.

On some systems it may become necessary to target a specific overlay plane through a pre-defined connector. Just forcing a layer index via `QT_QPA_EGLFS_LAYER_INDEX` does not perform plane configuration and is therefore not suitable in itself. Instead, in such special scenarios use the `QT_QPA_EGLFS_KMS_CONNECTOR_INDEX` and `QT_QPA_EGLFS_KMS_PLANE_INDEX` environment variables. When these are set, only the specified connector and plane will be in use, all other outputs will get ignored. The backend will take care of picking the EGL layer that corresponds to the desired plane, and the configuring of the plane.

### Touch input in systems with multiple screens on KMS/DRM

Touchscreens require additional considerations in multi-display systems because touch events have to be routed to the correct virtual screen, and this requires a correct mapping between touchscreens and display outputs.

The mapping is done via the JSON configuration file specified in `QT_QPA_EGLFS_KMS_CONFIG` and described in the previous sections. When a `touchDevice` property is present in an element of the `outputs` array, the value is treated as a device node and the touch device is associated with the display output in question.

For example, assuming our touchscreen has a device node of /dev/input/event5 and is a touchscreen integrated into the monitor connected via HDMI as the secondary screen, the following configuration ensures correct touch (and synthesized mouse) event translation:

       {
          "device": "drm-nvdc",
          "outputs": [
            {
              "name": "HDMI1",
              "touchDevice": "/dev/input/event5",
              "virtualIndex": 1
            },
            {
              "name": "DP1",
              "virtualIndex": 0
            }
          ]
      }

Note: When in doubt, enable logging from both the graphics and input subsystems by setting the environment variable `QT_LOGGING_RULES=qt.qpa.*=true` before launching the application. This will help identifying the correct input device nodes and may uncover output configuration issues that can be difficult to debug otherwise.

Note: As of Qt 5.8, the above is only supported for the evdevtouch input backend. Other variants, such as the libinput-based one, will continue to route events to the primary screen. To force the usage of evdevtouch on systems where multiple input backends are available, set the environment variable `QT_QPA_EGLFS_NO_LIBINPUT` to `1`.

### eglfs with other backends

Other backends, that are typically based on targeting the framebuffer or a composition API directly via the vendor's EGL implementation, usually provide limited or no support for multiple displays. On i.MX6-based boards with Vivante GPUs the `QT_QPA_EGLFS_FB` environment variable can be used to specify the framebuffer to target, similarly to linuxfb. On the Raspberry Pi the `QT_QPA_EGLFS_DISPMANX_ID` environment variable can be used to specify the screen to output to. The value corresponds to one of the `DISPMANX_ID_` constants, refer to the Dispmanx documentation. Note that these approaches, unlike KMS/DRM, will not typically allow to output to multiple screens from the same application. Alternatively, driver-specific environment variables or kernel parameters may also be available as well to control the used framebuffer. Refer to the embedded board's documentation.

### Video Memory

Systems with a fixed amount of dedicated video memory may need extra care before running Qt application based on Qt Quick or classes like QOpenGLWidget. The default setting may be insufficient for such applications, especially when they are displayed on a high resolution (for example, full HD) screen. In this case, they may start failing in unexpected ways. It is recommended to ensure that there is at least 128 MB of GPU memory available. For systems that do not have a fixed amount of memory reserved for the GPU this is not an issue.

### linuxfb

Use the `fb` plugin parameter to specify the framebuffer device to use.

## Unix Signal Handlers

The console-oriented platform plugins like eglfs and linuxfb install signal handlers by default to capture interrupt (`SIGINT`), suspend and continue (`SIGTSTP`, `SIGCONT`) and termination (`SIGTERM`). This way the keyboard, terminal cursor, and possibly other graphics state can be restored when the application terminates or gets suspended due to `kill`, or `Ctrl+C` or `Ctrl+Z`. (although terminating or suspending via the keyboard is only possible when `QT_QPA_ENABLE_TERMINAL_KEYBOARD` is set, as outlined above in the Input section). However, in some cases capturing `SIGINT` can be undesirable as it may conflict with remote debugging for instance. Therefore, the environment variable `QT_QPA_NO_SIGNAL_HANDLER` is provided to opt out from all built-in signal handling.

## Fonts

Qt normally uses `fontconfig` to provide access to system fonts. If `fontconfig` is not available, Qt will fall back to using `QBasicFontDatabase`. In this case, Qt applications will look for fonts in Qt's `lib/fonts` directory. Qt will automatically detect pre-rendered fonts and TrueType fonts. This directory can be overridden by setting the `QT_QPA_FONTDIR` environment variable.

For more information on the supported formats, see Qt for Embedded Linux Fonts.

Note: Qt no longer ships any fonts in the `lib/fonts` directory. This means that it is up to the platform (the system image) to provide the necessary fonts.

## Platform Plugins for Windowing Systems on Embedded Linux Devices

### XCB

This is the X11 plugin used on regular desktop Linux platforms. In some embedded environments, that provide X and the necessary development files for xcb, this plugin functions just like it does on a regular PC desktop.

Note: On some devices there is no EGL and OpenGL support available under X because the EGL implementation is not compatible with Xlib. In this case the XCB plugin is built without EGL support, meaning that Qt Quick 2 or other OpenGL-based applications does not work with this platform plugin. It can still be used however to run software-rendered applications (based on QWidget for example).

As a general rule, the usage of XCB on embedded devices is not advisable. Plugins like eglfs are likely to provide better performance, and hardware acceleration.

### Wayland

Wayland is a light-weight windowing system; or more precisely, it is a protocol for clients to talk to a display server.

Qt Wayland provides a `wayland` platform plugin that allows Qt applications to connect to a Wayland compositor.

For more details, see Wayland and Qt.

Note: You may experience issues with touch screen input while using the Weston reference compositor. For more information, see https://wiki.qt.io/WestonTouchScreenIssues.

## Related Topics

- Qt for Device Creation
- Configure an Embedded Linux Device
- Emulator
- Qt Virtual Keyboard
- Qt Quick WebGL