lwIP 2.2.0 Lightweight IP stack

Data Structures | Macros | Functions
mdns.c File Reference
`#include "lwip/apps/mdns.h"`
`#include "lwip/apps/mdns_priv.h"`
`#include "lwip/apps/mdns_domain.h"`
`#include "lwip/apps/mdns_out.h"`
`#include "lwip/netif.h"`
`#include "lwip/udp.h"`
`#include "lwip/ip_addr.h"`
`#include "lwip/mem.h"`
`#include "lwip/memp.h"`
`#include "lwip/prot/dns.h"`
`#include "lwip/prot/iana.h"`
`#include "lwip/timeouts.h"`
`#include "lwip/sys.h"`
`#include <string.h>`
`#include <stdio.h>`
`#include "lwip/igmp.h"`
`#include "lwip/mld6.h"`

## Data Structures
struct | mdns_packet

## Macros
#define | MDNS_RESPONSE_DELAY_MAX 120
#define | MDNS_PROBE_COUNT 3

## Functions
struct mdns_host * | netif_mdns_data (struct netif *netif)
struct udp_pcb * | get_mdns_pcb (void)
err_t | mdns_resp_add_netif (struct netif *netif, const char *hostname)
err_t | mdns_resp_remove_netif (struct netif *netif)
err_t | mdns_resp_rename_netif (struct netif *netif, const char *hostname)
int | mdns_resp_netif_active (struct netif *netif)
s8_t | mdns_resp_add_service (struct netif *netif, const char *name, const char *service, enum mdns_sd_proto proto, u16_t port, service_get_txt_fn_t txt_fn, void *txt_data)
err_t | mdns_resp_del_service (struct netif *netif, u8_t slot)
err_t | mdns_resp_rename_service (struct netif *netif, u8_t slot, const char *name)
err_t | mdns_resp_add_service_txtitem (struct mdns_service *service, const char *txt, u8_t txt_len)
void | mdns_search_stop (u8_t request_id)
err_t | mdns_search_service (const char *name, const char *service, enum mdns_sd_proto proto, struct netif *netif, search_result_fn_t result_fn, void *arg, u8_t *request_id)
void | mdns_resp_announce (struct netif *netif)
void | mdns_resp_register_name_result_cb (mdns_name_result_cb_t cb)
void | mdns_resp_restart_delay (struct netif *netif, uint32_t delay)
void | mdns_resp_restart (struct netif *netif)
void | mdns_resp_init (void)
void * | mdns_get_service_txt_userdata (struct netif *netif, s8_t slot)

## Detailed Description

MDNS responder implementation

## Macro Definition Documentation

## ◆ MDNS_PROBE_COUNT

#define MDNS_PROBE_COUNT 3

Probing & announcing defines

## ◆ MDNS_RESPONSE_DELAY_MAX

#define MDNS_RESPONSE_DELAY_MAX 120

Delayed response defines

## Function Documentation

## ◆ get_mdns_pcb()

struct udp_pcb* get_mdns_pcb | ( | void |  | ) |

Construction to access the mdns udp pcb.

Returns
  udp_pcb struct of mdns

## ◆ mdns_resp_register_name_result_cb()

void mdns_resp_register_name_result_cb | ( | mdns_name_result_cb_t | cb | ) |

Register a callback function that is called if probing is completed successfully or with a conflict.

## ◆ netif_mdns_data()

struct mdns_host* netif_mdns_data | ( | struct netif * | netif | ) |

Construction to make mdns struct accessible from mdns_out.c TODO: can we add the mdns struct to the netif like we do for dhcp, autoip,...? Then this is not needed any more.

Parameters

  netif | The network interface

Returns
  mdns struct