µracoli Arduino-Support-Package Version foo

- µracoli
- User Guide
- Reference Guide

Remote.ino

This sketch implements a COSM remote sensor, that measures temperature and VCC. The board sleeps during the idle period and is woken up by the watch dog.

/*
Cosm temperature logger
Remote node application
Hardware:
- Radiofaro on battery power, temperature sensor internal
*/
#include <avr/wdt.h>
#include <avr/sleep.h>
#include "HardwareRadio.h"
/* === globals ============================================================= */
static volatile uint8_t adcfinished = 0;
static int8_t adc_offset = 0;
/* === functions =========================================================== */
/*
* \brief Setup watchdog to serve as application timer
*
*/
static inline void wdt_timersetup(uint8_t timeout)
{
WDTCSR = (1 << WDCE) | (1 << WDE); /* Enable configuration change */
WDTCSR = (1 << WDIF) | (1 << WDIE) | /* Enable Watchdog Interrupt Mode */
(timeout & 0x08 ? _WD_PS3_MASK : 0x00) | (timeout & 0x07);
}
/*
* \brief Watchdog ISR, used as application timer
*
*/
ISR(WDT_vect, ISR_NOBLOCK)
{
/* do nothing, just wake up MCU */
}
ISR(ADC_vect, ISR_BLOCK)
{
adcfinished = 1;
}
/*
* \brief Trigger sleep based ADC measurement
* Function is blocking until flag "adcfinished" is set by ISR
*
* @return ADC register value
*/
static inline int16_t adc_measure(void)
{
set_sleep_mode(SLEEP_MODE_ADC);
/* dummy cycle */
adcfinished = 0;
do
{
sleep_mode();
/* sleep, wake up by ADC IRQ */
/* check here for ADC IRQ because sleep mode could wake up from
* another source too
*/
} while (0 == adcfinished); /* set by ISR */
return ADC ;
}
float measure_tmcu(void)
{
int32_t val = 0;
uint8_t nbavg = 5;
ADCSRA = (1 << ADEN) | (1 << ADPS2) | (1 << ADPS1); /* PS 64 */
ADCSRB = (1 << MUX5);
ADMUX = (1 << REFS1) | (1 << REFS0) | (1 << MUX3) | (1 << MUX0); /* reference: 1.6V, input Temp Sensor */
_delay_us(200); /* some time to settle */
ADCSRA |= (1 << ADIF); /* clear flag */
ADCSRA |= (1 << ADIE);
/* dummy cycle after REF change (suggested by datasheet) */
adc_measure();
_delay_us(100); /* some time to settle */
for(uint8_t i=0;i<nbavg;i++){
val += adc_measure() - adc_offset;
}
ADCSRA &= ~((1 << ADEN) | (1 << ADIE));
return (1.13 * val / (float)nbavg - 272.8);
}
int8_t measure_adc_offset(void)
{
uint16_t val;
ADCSRA = (1 << ADEN) | (1 << ADPS2) | (1 << ADPS1); /* PS 64 */
ADCSRB = 0;
ADMUX = (1 << REFS1) | (1 << REFS0) | (1 << MUX3); /* reference: 1.6V, differential ADC0-ADC0 10x */
_delay_us(200); /* some time to settle */
ADCSRA |= (1 << ADIF); /* clear flag */
ADCSRA |= (1 << ADIE);
/* dummy cycle after REF change (suggested by datasheet) */
adc_measure();
_delay_us(100); /* some time to settle */
val = adc_measure();
ADCSRA &= ~((1 << ADEN) | (1 << ADIE));
return (val);
}
/*
* \brief Measure internal voltage of ATmega128RFA1
*
* Cannot be measured via ADC, use Batmon of TRX part
*
*/
float measure_vmcu(void)
{
uint16_t v; /* voltage in [mV] */
uint8_t vth;
for(vth=0;vth<32;vth++){
BATMON = vth & 0x1F;
BATMON = vth & 0x1F;
if(0 == (BATMON & (1<<BATMON_OK))){
break;
}
}
if(vth & 0x10){
v = 2550 + 75*(vth&0x0F); /* high range */
}else{
v = 1700 + 50*(vth&0x0F); /* low range */
}
return v / 1000.0;
}
void setup()
{
/* init all unused pins */
DDRB = 0x00; /* as input */
PORTB = 0xFF; /* pullups */
DDRD = 0x00; /* as input */
PORTD = 0xFF; /* pullups */
DDRE = 0x00; /* as input */
PORTE = 0xFF; /* pullups */
DDRF = 0x00; /* as input */
PORTF = 0xFF; /* pullups */
DDRG = 0x00; /* as input */
PORTG = 0xFF; /* pullups */
DIDR0 = 0xFF; /* disable all ADC inputs */
/* we are using async Tx only, never receive
* anything. Therefore we choose sleep as idle state
*/
Radio.begin(17, STATE_SLEEP);
adc_offset = measure_adc_offset();
wdt_timersetup(WDTO_8S);
set_sleep_mode(SLEEP_MODE_PWR_DOWN);
}
void loop()
{
float tmcu, vmcu;
tmcu = measure_tmcu();
vmcu = measure_vmcu();
Radio.print("ADDR=");
Radio.print(Radio.nc.short_addr);
Radio.print(", T=");
Radio.print(tmcu);
Radio.print(", V=");
Radio.print(vmcu);
Radio.print('\n');
Radio.flush();
while(Radio.tx_in_progress);
set_sleep_mode(SLEEP_MODE_PWR_DOWN);
sleep_mode();
}