µracoli Arduino-Support-Package Version foo

- µracoli
- User Guide
- Reference Guide

HelloRadio.ino

This sketch sends frames with a period of 500ms.

/* $Id$ */
#include "HardwareRadio.h"
#define REG(name, reg) do{uint8_t _b_ = reg; Serial.print(name);Serial.print(" : "); Serial.println(_b_,HEX);}while(0)
unsigned long tx_time;
int cnt = 0;
void setup() {
/* operating on channel 17, not receiving when idle. */
Radio.begin(17, STATE_OFF);
Serial.begin(57600);
Serial.println("HelloRadio V$Release$");
}
void loop() {
if (millis() > tx_time){
tx_time = millis() + 500;
// write string
Radio.write("cnt: ");
// write integer
Radio.print(cnt);
// write byte
Radio.write('\n');
Radio.flush();
Serial.println(cnt);
cnt ++;
}
}