µracoli Arduino-Support-Package Version foo

- µracoli
- User Guide
- Reference Guide

IoCheck.ino

This is sketch performs a simple GPIO check, no radio functions included.

/* $Id$ */
#include "HardwareRadio.h"
bool DO_ECHO = false;
void setup()
{
Serial.begin(57600);
// flush input
while(Serial.available())
{
Serial.read();
}
Radio.begin();
Serial.println("Sketch IoCheck\n\r"
"Type help for a list of commands");
}
void loop()
{
static uint8_t val = 0;
static char line[32], *pcmd;
if (DO_ECHO)
{
Serial.print("\n\rIoCheck>");
}
/* check serial IO */
pcmd = readline(line, sizeof(line));
if(pcmd != NULL)
{
if (DO_ECHO)
{
Serial.println(pcmd);
}
process_command(pcmd);
}
}
// =============================================================
// parse command and dispatch to execution function
void process_command(char *pcmd)
{
char *argv[8], *p;
int argc = 0, i;
bool newarg;
p = pcmd;
argv[argc++] = p;
newarg = false;
while(*p != 0)
{
if (*p == ' ')
{
*p = 0;
newarg = true;
}
else
{
if (newarg == true && argc < 8)
{
argv[argc++] = p;
newarg = false;
}
}
p++;
}
#if 0
// dump result of line parsing
for (i=0; i<argc; i++)
{
Serial.print(" - ");
Serial.print(i);
Serial.print(":");
Serial.println(argv[i]);
}
#endif
if (strncasecmp("pin", argv[0], 3) == 0)
{
execute_pin_command(argv + 1, argc - 1);
}
else if (strncasecmp("help", argv[0], 4) == 0)
{
execute_print_help();
}
else if (strncasecmp("echo", argv[0], 4) == 0)
{
DO_ECHO = atoi(argv[1]) ? true : false;
Serial.print("echo is now ");
Serial.println(DO_ECHO ? "ON": "OFF");
}
else if (strncasecmp("jtag", argv[0], 4) == 0)
{
execute_set_jtag(atoi(argv[1]) ? true : false);
}
else if (strncasecmp("sleep", argv[0], 4) == 0)
{
execute_set_sleep();
}
else if (strncasecmp("tx", argv[0], 2) == 0)
{
execute_transmit();
}
else if (strncasecmp("rx", argv[0], 2) == 0)
{
execute_receive(atoi(argv[1]));
}
}
void execute_print_help(void)
{
Serial.print("\n\r"
" pin <id> <dir> <val> : set pin (id is e.g. 'd0' or 'a0', dir: 0=input, 1=output)\n\r"
" echo <bool> : switch echo ON/OFF\n\r"
" jtag <bool> : switch jtag ON/OFF\n\r"
" sleep : set MCU and TRX to sleep\n\r"
" tx : transmit frame\n\r"
" rx <tmo> : receive frame (tmo to wait for frame in ms)\n\r"
" help : print help\n\r");
}