µracoli Arduino-Support-Package Version foo

- µracoli
- User Guide
- Reference Guide

Boards and Modules

# atzb256rfr2xpro

Board #1: Atmel ATmega256RFR2 ZigBit Xplained Pro Extension

Board atzb256rfr2xpro

Parameters

- Build Target: `atzb256rfr2xpro`
- Build Aliases: secatrcb256rfr2xpro
- Include file: `board_derfa.h`
- Baudrate: `57600`
- MMCU: `atmega256rfr2`
- F_CPU: `16000000UL`
- Provides: `hif, key, led, mcu_t, mcu_vtg, rtc, sensors, tmr, trx`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_key_events, xmpl_keys, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# mnb900

Board #2: Meshnetics MeshBean WDB-A1281 and MNZB-900 development boards

Board mnb900

Parameters

- Build Target: `mnb900`
- Include file: `board_wdba1281.h`
- Baudrate: `38400`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `ds18b20, hif, i2c, led, lm73, mcu_vtg, ow, rtc, sensors, tmr, trx, trxvtg, tsl2550`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_i2c, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_lm73, xmpl_ow, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret, xmpl_tsl2550

# pinoccio

Board #3: Pinoccio - the ecosystem for the internet of things

Board pinoccio

Parameters

- Build Target: `pinoccio`
- Include file: `board_derfa.h`
- Baudrate: `115200`
- MMCU: `atmega256rfr2`
- F_CPU: `16000000UL`
- Fuses: `-U lfuse:w:0xf7:m -U hfuse:w:0xda:m -U efuse:w:0xf5:m`
- Provides: `hif, led, mcu_t, mcu_vtg, rtc, sensors, tmr, trx`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# radiofaro

Board #4: RadioFaro, Arduino like board with deRFmega128-22A001

Board radiofaro

Parameters

- Build Target: `radiofaro`
- Include file: `board_derfa.h`
- Baudrate: `57600`
- MMCU: `atmega128rfa1`
- F_CPU: `16000000UL`
- Fuses: `-U lfuse:w:0xf7:m -U hfuse:w:0x9a:m -U efuse:w:0xfe:m`
- Provides: `hif, led, mcu_t, mcu_vtg, rtc, sensors, tmr, trx, trxvtg`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret

# wdba1281

Board #5: Meshnetics MeshBean WDB-A1281 and MNZB-900 development boards

Board wdba1281

Parameters

- Build Target: `wdba1281`
- Build Aliases: mnb900
- Include file: `board_wdba1281.h`
- Baudrate: `38400`
- MMCU: `atmega1281`
- F_CPU: `8000000UL`
- Provides: `ds18b20, hif, i2c, led, lm73, mcu_vtg, ow, rtc, sensors, tmr, trx, trxvtg, tsl2550`

Applications

diag, rdiag, rsensor, selftest, sniffer, testlib, wgpio, wibo, wibohost, wibotest, wuart

Examples

xmpl_dbg, xmpl_hif, xmpl_hif_echo, xmpl_i2c, xmpl_leds, xmpl_linbuf_rx, xmpl_linbuf_tx, xmpl_lm73, xmpl_ow, xmpl_radio_range, xmpl_radio_stream, xmpl_rtc, xmpl_sensor, xmpl_timer, xmpl_timer_callback, xmpl_trx_base, xmpl_trx_echo, xmpl_trx_rx, xmpl_trx_rxaack, xmpl_trx_tx, xmpl_trx_txaret, xmpl_tsl2550