this is the last issue of alt-1 you will ever see hahahahaha no more!  there
will be no more since we couldn't even get enough fucking articles for 3
sections without digging into old alt-1s.  so forget it.  fuck you all. go to
hell and burn there for all i care.  just FUCK OFF .  eternal darkness swallow
you all.

ems used for buffering uncompressed bitmaps (as opposed to decompressing them
        again) :)  ems is checked...as well as available mem...128k needed...
svga 1024x768x256 mode supported through VESA bios extensions (does not check
        for valid vesa bios...sorry)
GUS required for sound, optional EMS use...MIDAS can put patterns and shit into
        ems if you have it...this hacked version of midas uses the LAPD file
        system and has everything except s3m and gus removed... :) whee...
LAPD used for all files and shit, so everything can be appended to the EXE,
        compressed and encoded.  nice, eh?  well..kinda...needs some more work
        before it's a real loader tho...
        (lapd = lithiums archive packer/depacker)
UMBs are now allocated before conventional memory...

