
The emulator is DCMOTO

The emulator can be downloaded from the following link: http://dcmoto.free.fr/emulateur/index.html

CONFIGURE THE EMULATOR
At startup the emulator is configured to emulate the TO9 + computer and the interface is in French.
To change the emulated computer and language click on the OPTIONS menu.
A window appears with several boxes containing various items.
From the first panel (ordinateur) select MO6 or PC128 olivetti (they are the same)
To change the language select it from the Langue box
The Joystick is emulated by holding down CTRL + the UP, LEFT, DOWN, RIGHT arrow keys and SPACE for FIRE
ATTENTION the Joystick emulation probably has a BUG, ​​sometimes the direction remains blocked as if the button was pressed.
To avoid this you can disable the emulation of the joystick by removing the check from the checkbox (Ctrl + Up ...) and setting the joystick from the TOOLS menu item JOYSTICK


INSTRUCTIONS FOR LOADING THE K7 FILE (BASIC LIST)
1 - open the REMOVABLE MEDIA menu
2 - click on the LOAD button of the TAPE(K7) area and select the happy10th.k7 file
2 - in the start screen select 1 BASIC 128 Microsoft 1.0 to enter the BASIC 
(by clicking on the yellow rectangle or by pressing the 1 key)
3 - type LOAD once loading is completed type RUN to start the program or LIST to see the listing.

** Another possibility is to directly load the source text file **
1 - in the start screen select 1 BASIC 128 Microsoft 1.0 to enter the BASIC
2 - click on the FILE menu
3 - select the item "Simulate Keyboard"
4 - Browse the file Source-code.txt
5 - Click on the "Simulate with the text file" button and the file is listed in the editor

For game instructions see the file Game-istruction.txt

For any problem please contact me at the following address: pestassi@gmail.com



