Minim core | ugens | analysis |
Gain gain | Description The gain input controls the value of this Gain. It will be interpreted as being in dB. 0 dB means that the incoming signal will not be changed, positive dB increases the amplitude of the signal, and negative dB decreases it. You can effectively silence the incoming signal by setting the gain to something like -60. Signature
    UGen.UGenInput gain
Related Gain Example
    None available
Usage Web & Application