Building U-Boot Image | Qt 5.12

- Qt 5.12
- Building U-Boot Image
- Qt 5.12.9 Reference Documentation

Building Monolith Project ◦ Creating Bootable SD Card

# Building U-Boot Image

To build a U-Boot image, open a terminal and navigate to the project directory created in Building Monolith Project. In our example the project directory is mymonolith.

Under the project directory, you will find an executable with the same name you gave to your monolith in Project Manager Settings. In our example the executable name is myproject.

Run the `elfloader` command for the executable. You will find the `elfloader` command under your compiler directory:

     john@doe: /usr/ghs/comp_201654/elfloader -l /usr/ghs/int1144/util/elfloader/cortexa9_elfloader.bin -o myproject.elf myproject

The example `elfloader` command above assumes your Green Hills Software (GHS) compiler is version 2016.5.4, and your INTEGRITY and GHS compiler installations are found from their default locations. However, you can modify the paths in the example according to your configuration.

Finally, build the U-Boot image with the `mkimage` tool. The last argument in the `mkimage` command specifies the U-Boot image name. In the example below, we use the name demo.image. To invoke `mkimage`, run the following command in a terminal:

     john@doe: mkimage -A arm -O linux -T kernel -C none -a 20000000 -e 20000000 -n INTEGRITY+Qt -d myproject.elf demo.image

Building Monolith Project ◦ Creating Bootable SD Card