lwIP 2.2.0 Lightweight IP stack

Modules | Data Structures | Functions
TFTP client/server
Applications

## Modules
| Options

## Data Structures
struct | tftp_context

## Functions
err_t | tftp_init_server (const struct tftp_context *ctx)
err_t | tftp_init_client (const struct tftp_context *ctx)
void | tftp_cleanup (void)

## Detailed Description

This is simple TFTP client/server for the lwIP raw API. You need to increase MEMP_NUM_SYS_TIMEOUT by one if you use TFTP!

## Function Documentation

## ◆ tftp_cleanup()

void tftp_cleanup | ( | void |  | ) |

Deinitialize ("turn off") TFTP client/server.

## ◆ tftp_init_client()

err_t tftp_init_client | ( | const struct tftp_context * | ctx | ) |

Initialize TFTP client.

Parameters

  ctx | TFTP callback struct

## ◆ tftp_init_server()

err_t tftp_init_server | ( | const struct tftp_context * | ctx | ) |

Initialize TFTP server.

Parameters

  ctx | TFTP callback struct