Minim core | ugens | analysis |
Waves pulse | Description Constructs a perfect square wave with the specified duty cycle. Signature
    Wavetable pulse(float dutyCycle)
Parameters dutyCycle — float: a square wave with a duty cycle of 0.5 will be a perfect square wave that is 1 half the time and -1 the other half. By changing the duty cycle, you change how much of the square is below zero. So, a duty cycle of 0.2 would result in 20 percent of the square below zero and the rest above. Duty cycle will be clamped to [0,1]. Returns Wavetable Related Waves Wavetable Waveform Example
    None available
Usage Web & Application