Minim core | ugens | analysis |
FourierTransform inverse | Description Performs an inverse transform of the frequency spectrum and places the result in `buffer`. Signature
    void inverse(float[] buffer)
    void inverse(AudioBuffer buffer)
    void inverse(float[] freqReal, float[] freqImag, float[] buffer)
Parameters buffer — float[]: the buffer to place the result of the inverse transform in buffer — AudioBuffer: the buffer to place the result of the inverse transform in freqReal — float[]: the real part of the frequency spectrum freqImag — float[]: the imaginary part the frequency spectrum buffer — float[]: the buffer to place the inverse transform in Returns None Related FFT Example
    None available
Usage Web & Application